Problem 7

Number of needed subnets 2000

Number of needed usable hosts 15

Network Address 178.100.0.0

Address class B

Default subnet mask 255.255.0.0

Custom subnet mask 255.255.255.224

Total number of subnets 2048

Total number of hosts addresses 32

Number of usable addresses 30

Number of bits borrowed 11